
A blue and white logo

Description automatically generated

Three **Kawasaki 1100s** were coated with Sea-Slide® and below are the results:

All tests were one hour long in duration.



|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Test** | **Water Conditions** | **Fuel Consumption** | **Top Speed** | **Handling** |
| 1 | Calm | .5 gals | 60 mph | Excellent |
| 2 | Slight Chop | 1.25 gals | 50 mph | Good |
| 3 | Choppy | 2.0 gals | 45 mph | Fair |



|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Subject #** | **Water Conditions** | **Fuel Consumption** | **Top Speed** | **Handling** |
| 1 | Calm | <.25 gals | >65 mph | Excellent |
| 1 | Slight Chop | .75 gals | >65 mph | Very Good |
| 1 | Choppy | 1.0 gals | 60 mph | Very Good |



|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Subject #** | **Water Conditions** | **Fuel Consumption** | **Top Speed** | **Handling** |
| 2 | Calm | <.25 gals | >65 mph | Excellent |
| 2 | Slight Chop | 1.0 gals | 65 mph | Very Good |
| 2 | Choppy | .75 gals | 57 mph | Excellent |



|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Subject #** | **Water Conditions** | **Fuel Consumption** | **Top Speed** | **Handling** |
| 3 | Calm | <.25 gals | >65 mph | Excellent |
| 3 | Slight Chop | <1.25 gals | >65 mph | Excellent |
| 3 | Choppy | 1.0 gals | 65 mph | Good |

>65 means that they buried their speedometers!

Durability - all subjects reported that one coating lasted more than 2 weeks.

Ease of application ranged from Very Good to Excellent.

All subjects noted that when left in the water, the watercraft had substantial fouling when uncoated. When coated, minimum fouling was noticed, even when left in the water for two weeks.

A qr code with blue text

Description automatically generated

All subjects noted that they would purchase Sea-Slide if available for personal use.

Please contact:

[p/mccue@hydromer.com](mailto:p/mccue@hydromer.com)